HME(4) | Device Drivers Manual | HME(4)

# NAME

`hme` — Sun Happy Meal 10/100 Ethernet device

# SYNOPSIS

`hme* at pci?`
`hme* at sbus?`
`luphy* at mii?`
`nsphy* at mii?`
`qsphy* at mii?`

# DESCRIPTION

The `hme` driver provides support for various NICs based on the Sun Happy Meal Ethernet controller chips, including the following:

- Sun FastEthernet PCI
- Sun FastEthernet SBus
- Sun Quad FastEthernet PCI
- Sun Quad FastEthernet SBus
- Sun SunSwift PCI
- Sun SunSwift SBus

The `hme` driver supports several media types, which are selected via the ifconfig(8) command. The supported media types are:

media autoselect
  Attempt to autoselect the media type (default)
media 100baseTX mediaopt full-duplex
  Use 100baseTX, full duplex
media 100baseTX
  Use 100baseTX, half duplex
media 10baseT mediaopt full-duplex
  Use 10baseT, full duplex
media 10baseT
  Use 10baseT, half duplex

# SEE ALSO

arp(4), ifmedia(4), inet(4), intro(4), luphy(4), netintro(4), nsphy(4), qsphy(4), sbus(4), hostname.if(5), ifconfig(8)

Sun Microelectronics, STP2002QFP Fast Ethernet, Parallel Port, SCSI (FEPS) User's Guide, April 1996.

# HISTORY

OpenBSD support for the `hme` first appeared in OpenBSD 2.4.

November 5, 2019 | Debian