BGW(4) | Device Drivers Manual | BGW(4)

# NAME

`bgw` — Bosch motion sensor

# SYNOPSIS

`bgw* at iic?`

# DESCRIPTION

The `bgw` driver provides support for the Bosch BMC150, BMI055, BMA222E, BMA250E, BMA255 and BMA280 motion sensors. The acceleration data as well as the chip temperature are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `bgw` driver first appeared in OpenBSD 6.3.

# AUTHORS

The `bgw` driver was written by Mark Kettenis <kettenis@openbsd.org>.

November 30, 2017 | Debian