VTE(4) | Device Drivers Manual | VTE(4)

# NAME

`vte` — RDC R6040 10/100 Ethernet device

# SYNOPSIS

`vte* at pci?`
`rdcphy* at mii?`

# DESCRIPTION

The `vte` driver provides support for Ethernet interfaces based on the RDC R6040 Ethernet chipset which is commonly found on Vortex86 System On a Chip (SoC).

The `vte` driver supports interrupt moderation mechanism, a 64-bit multicast hash filter.

The following media types are supported:

`autoselect`
  Enable autoselection of the media type and options.
`10baseT`
  Set 10Mbps operation.
`100baseTX`
  Set 100Mbps (Fast Ethernet) operation.

For more information on configuring this device, see ifconfig(8). To view a list of media types and options supported by the card, try `ifconfig <device> media`. For example, `ifconfig vte0 media`.

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), pci(4), rdcphy(4), hostname.if(5), ifconfig(8)

# HISTORY

The `vte` device driver first appeared in OpenBSD 4.9.

# AUTHORS

The `vte` driver was written by Pyun YongHyeon for FreeBSD and ported to OpenBSD by Kevin Lo <kevlo@openbsd.org>.

July 16, 2013 | Debian