TERMIOS(4) | Device Drivers Manual | TERMIOS(4)

# NAME

`termios` — general terminal line discipline

# SYNOPSIS

`#include <termios.h>`

# DESCRIPTION

This describes a general terminal line discipline that is supported on tty asynchronous communication ports.

## Opening a Terminal Device File

When a terminal file is opened, it normally causes the process to wait until a connection is established. For most hardware, the presence of a connection is indicated by the assertion of the hardware `CARRIER line`. If the termios structure associated with the terminal file has the `CLOCAL` flag set in the cflag, or if the `O_NONBLOCK` flag is set in the open(2) call, then the open will succeed even without a connection being present. In practice, applications seldom open these files; they are opened by special programs, such as getty(8) or sshd(8), and become an application's standard input, output, and error files.

## Job Control in a Nutshell

Every process is associated with a particular process group and session. The grouping is hierarchical: every member of a particular process group is a member of the same session. This structuring is used in managing groups of related processes for purposes of job control; that is, the ability from the keyboard (or from program control) to simultaneously stop or restart a complex command (a command composed of one or more related processes). The grouping into process groups allows delivering of signals that stop or start the group as a whole, along with arbitrating which process group has access to the single controlling terminal. The grouping at a higher layer into sessions is to restrict the job control related signals and system calls to within processes resulting from a particular instance of a "login". Typically, a session is created when a user logs in, and the login terminal is set up to be the controlling terminal; all processes spawned from that login shell are in the same session, and inherit the controlling terminal. A job control shell operating interactively (that is, reading commands from a terminal) normally groups related processes together by placing them into the same process group. A set of processes in the same process group is collectively referred to as a "job". When the foreground process group of the terminal is the same as the process group of a particular job, that job is said to be in the "foreground". When the process group of the terminal is different than the process group of a job (but is still the controlling terminal), that job is said to be in the "background". Normally the shell reads a command and starts the job that implements that command. If the command is to be started in the foreground (typical), it sets the process group of the terminal to the process group of the started job, waits for the job to complete, and then sets the process group of the terminal back to its own process group (it puts itself into the foreground). If the job is to be started in the background (as denoted by the shell operator "&"), it never changes the process group of the terminal and doesn't wait for the job to complete (that is, it immediately attempts to read the next command). If the job is started in the foreground, the user may type a key (usually ‘`^Z`’) which generates the terminal stop signal (`SIGTSTP`) and has the effect of stopping the entire job. The shell will notice that the job stopped, and will resume running after placing itself in the foreground. The shell also has commands for placing stopped jobs in the background, and for placing stopped or background jobs into the foreground.

## Orphaned Process Groups

An orphaned process group is a process group that has no process whose parent is in a different process group, yet is in the same session. Conceptually it means a process group that doesn't have a parent that could do anything if it were to be stopped. For example, the initial login shell is typically in an orphaned process group. Orphaned process groups are immune to keyboard generated stop signals and job control signals resulting from reads or writes to the controlling terminal.

## The Controlling Terminal

A terminal may belong to a process as its controlling terminal. Each process of a session that has a controlling terminal has the same controlling terminal. A terminal may be the controlling terminal for at most one session. The controlling terminal for a session is allocated by the session leader by issuing the `TIOCSCTTY` ioctl. A controlling terminal is never acquired by merely opening a terminal device file. When a controlling terminal becomes associated with a session, its foreground process group is set to the process group of the session leader.

The controlling terminal is inherited by a child process during a fork(2) function call. A process relinquishes its controlling terminal when it creates a new session with the setsid(2) function; other processes remaining in the old session that had this terminal as their controlling terminal continue to have it. A process does not relinquish its controlling terminal simply by closing all of its file descriptors associated with the controlling terminal if other processes continue to have it open.

When a controlling process terminates, the controlling terminal is disassociated from the current session, allowing it to be acquired by a new session leader. Subsequent access to the terminal by other processes in the earlier session will be denied, with attempts to access the terminal treated as if modem disconnect had been sensed.

## Terminal Access Control

If a process is in the foreground process group of its controlling terminal, read operations are allowed. Any attempts by a process in a background process group to read from its controlling terminal causes a `SIGTTIN` signal to be sent to the process's group unless one of the following special cases apply: If the reading process is ignoring or blocking the `SIGTTIN` signal, or if the process group of the reading process is orphaned, the read(2) returns -1 with errno set to `EIO` and no signal is sent. The default action of the `SIGTTIN` signal is to stop the process to which it is sent.

If a process is in the foreground process group of its controlling terminal, write operations are allowed. Attempts by a process in a background process group to write to its controlling terminal will cause the process group to be sent a `SIGTTOU` signal unless one of the following special cases apply: If `TOSTOP` is not set, or if `TOSTOP` is set and the process is ignoring or blocking the `SIGTTOU` signal, the process is allowed to write to the terminal and the `SIGTTOU` signal is not sent. If `TOSTOP` is set, and the process group of the writing process is orphaned, and the writing process is not ignoring or blocking `SIGTTOU`, the write(2) returns -1 with errno set to `EIO` and no signal is sent.

Certain calls that set terminal parameters are treated in the same fashion as write, except that `TOSTOP` is ignored; that is, the effect is identical to that of terminal writes when `TOSTOP` is set.

## Input Processing and Reading Data

A terminal device associated with a terminal device file may operate in full-duplex mode, so that data may arrive even while output is occurring. Each terminal device file has associated with it an input queue, into which incoming data is stored by the system before being read by a process. The system imposes a limit, `MAX_INPUT`, on the number of bytes that may be stored in the input queue. The behavior of the system when this limit is exceeded depends on the setting of the `IMAXBEL` flag in the termios c_iflag. If this flag is set, the terminal is sent an ASCII BEL character each time a character is received while the input queue is full. Otherwise, the input queue is flushed upon receiving the character.

Two general kinds of input processing are available, determined by whether the terminal device file is in canonical mode or noncanonical mode. Additionally, input characters are processed according to the c_iflag and c_lflag fields. Such processing can include echoing, which in general means transmitting input characters immediately back to the terminal when they are received from the terminal. This is useful for terminals that can operate in full-duplex mode.

The manner in which data is provided to a process reading from a terminal device file is dependent on whether the terminal device file is in canonical or noncanonical mode.

Another dependency is whether the `O_NONBLOCK` flag is set by `open`() or `fcntl`(). If the `O_NONBLOCK` flag is clear, then the read request is blocked until data is available or a signal has been received. If the `O_NONBLOCK` flag is set, then the read request is completed, without blocking, in one of three ways:

1. If there is enough data available to satisfy the entire request, and the read completes successfully the number of bytes read is returned.
2. If there is not enough data available to satisfy the entire request, and the read completes successfully, having read as much data as possible, the number of bytes read is returned.
3. If there is no data available, the read returns -1, with errno set to `EAGAIN`.

When data is available depends on whether the input processing mode is canonical or noncanonical.

## Canonical Mode Input Processing

In canonical mode input processing, terminal input is processed in units of lines. A line is delimited by a newline ‘`\n`’ character, an end-of-file (`EOF`) character, or an end-of-line (`EOL`) character. See the Special Characters section for more information on `EOF` and `EOL`. This means that a read request will not return until an entire line has been typed, or a signal has been received. Also, no matter how many bytes are requested in the read call, at most one line is returned. It is not, however, necessary to read a whole line at once; any number of bytes, even one, may be requested in a read without losing information.

`MAX_CANON` is a limit on the number of bytes in a line. The behavior of the system when this limit is exceeded is the same as when the input queue limit `MAX_INPUT`, is exceeded.

Erase and kill processing occur when either of two special characters, the `ERASE` and `KILL` characters (see the Special Characters section), is received. This processing affects data in the input queue that has not yet been delimited by a newline `NL`, `EOF`, or `EOL` character. This un-delimited data makes up the current line. The `ERASE` character deletes the last character in the current line, if there is any. The `KILL` character deletes all data in the current line, if there is any. The `ERASE` and `KILL` characters have no effect if there is no data in the current line. The `ERASE` and `KILL` characters themselves are not placed in the input queue.

## Noncanonical Mode Input Processing

In noncanonical mode input processing, input bytes are not assembled into lines, and erase and kill processing does not occur. The values of the `VMIN` and `VTIME` members of the c_cc array are used to determine how to process the bytes received.

`VMIN` represents the minimum number of bytes that should be received when the read(2) function successfully returns. `VTIME` is a timer of 0.1 second granularity that is used to time out bursty and short term data transmissions. If `VMIN` is greater than `MAX_INPUT`, the response to the request is undefined. The four possible values for `VMIN` and `VTIME` and their interactions are described below.

## Case A: VMIN > 0, VTIME > 0

In this case `VTIME` serves as an inter-byte timer and is activated after the first byte is received. Since it is an inter-byte timer, it is reset after a byte is received. The interaction between `VMIN` and `VTIME` is as follows: as soon as one byte is received, the inter-byte timer is started. If `VMIN` bytes are received before the inter-byte timer expires (remember that the timer is reset upon receipt of each byte), the read is satisfied. If the timer expires before `VMIN` bytes are received, the characters received to that point are returned to the user. Note that if `VTIME` expires at least one byte is returned because the timer would not have been enabled unless a byte was received. In this case (`VMIN` > 0, `VTIME` > 0) the read blocks until the `VMIN` and `VTIME` mechanisms are activated by the receipt of the first byte, or a signal is received. If data is in the buffer at the time of the read(), the result is as if data had been received immediately after the read().

## Case B: VMIN > 0, VTIME = 0

In this case, since the value of `VTIME` is zero, the timer plays no role and only `VMIN` is significant. A pending read is not satisfied until `VMIN` bytes are received (i.e., the pending read blocks until `VMIN` bytes are received), or a signal is received. A program that uses this case to read record-based terminal I/O may block indefinitely in the read operation.

## Case C: VMIN = 0, VTIME > 0

In this case, since `VMIN` = 0, `VTIME` no longer represents an inter-byte timer. It now serves as a read timer that is activated as soon as the read function is processed. A read is satisfied as soon as a single byte is received or the read timer expires. Note that in this case if the timer expires, no bytes are returned. If the timer does not expire, the only way the read can be satisfied is if a byte is received. In this case the read will not block indefinitely waiting for a byte; if no byte is received within `VTIME`*0.1 seconds after the read is initiated, the read returns a value of zero, having read no data. If data is in the buffer at the time of the read, the timer is started as if data had been received immediately after the read.

## Case D: VMIN = 0, VTIME = 0

The minimum of either the number of bytes requested or the number of bytes currently available is returned without waiting for more bytes to be input. If no characters are available, read returns a value of zero, having read no data.

## Writing Data and Output Processing

When a process writes one or more bytes to a terminal device file, they are processed according to the c_oflag field (see the Output Modes section). The implementation may provide a buffering mechanism; as such, when a call to write() completes, all of the bytes written have been scheduled for transmission to the device, but the transmission will not necessarily have been completed.

## Special Characters

Certain characters have special functions on input or output or both. These functions are summarized as follows:

`INTR`
  Special character on input and is recognized if the `ISIG` flag (see the Local Modes section) is enabled. Generates a `SIGINT` signal which is sent to all processes in the foreground process group for which the terminal is the controlling terminal. If `ISIG` is set, the `INTR` character is discarded when processed.
`QUIT`
  Special character on input and is recognized if the `ISIG` flag is enabled. Generates a `SIGQUIT` signal which is sent to all processes in the foreground process group for which the terminal is the controlling terminal. If `ISIG` is set, the `QUIT` character is discarded when processed.
`ERASE`
  Special character on input and is recognized if the `ICANON` flag is set. Erases the last character in the current line; see Canonical Mode Input Processing. It does not erase beyond the start of a line, as delimited by a `NL`, `EOF`, or `EOL` character. If `ICANON` is set, the `ERASE` character is discarded when processed.
`KILL`
  Special character on input and is recognized if the `ICANON` flag is set. Deletes the entire line, as delimited by a `NL`, `EOF`, or `EOL` character. If `ICANON` is set, the `KILL` character is discarded when processed.
`EOF`
  Special character on input and is recognized if the `ICANON` flag is set. When received, all the bytes waiting to be read are immediately passed to the process, without waiting for a newline, and the `EOF` is discarded. Thus, if there are no bytes waiting (that is, the `EOF` occurred at the beginning of a line), a byte count of zero is returned from the read(), representing an end-of-file indication. If `ICANON` is set, the `EOF` character is discarded when processed.
`NL`
  Special character on input and is recognized if the `ICANON` flag is set. It is the line delimiter ‘`\n`’.
`EOL`
  Special character on input and is recognized if the `ICANON` flag is set. Is an additional line delimiter, like `NL`.
`SUSP`
  If the `ISIG` flag is enabled, receipt of the `SUSP` character causes a `SIGTSTP` signal to be sent to all processes in the foreground process group for which the terminal is the controlling terminal, and the `SUSP` character is discarded when processed.
`STOP`
  Special character on both input and output and is recognized if the `IXON` (output control) or `IXOFF` (input control) flag is set. Can be used to temporarily suspend output. It is useful with fast terminals to prevent output from disappearing before it can be read. If `IXON` is set, the `STOP` character is discarded when processed.
`START`
  Special character on both input and output and is recognized if the `IXON` (output control) or `IXOFF` (input control) flag is set. Can be used to resume output that has been suspended by a `STOP` character. If `IXON` is set, the `START` character is discarded when processed.
`CR`
  Special character on input and is recognized if the `ICANON` flag is set; it is the ‘`\r`’, as denoted in the C Standard {2}. When `ICANON` and `ICRNL` are set and `IGNCR` is not set, this character is translated into a `NL`, and has the same effect as a `NL` character.

The following special characters are extensions defined by this system and are not a part of 1003.1 termios.

`EOL2`
  Secondary `EOL` character. Same function as `EOL`.
`WERASE`
  Special character on input and is recognized if the `ICANON` flag is set. Erases the last word in the current line according to one of two algorithms. If the `ALTWERASE` flag is not set, first any preceding whitespace is erased, and then the maximal sequence of non-whitespace characters. If `ALTWERASE` is set, first any preceding whitespace is erased, and then the maximal sequence of alphabetic/underscores or non alphabetic/underscores. As a special case in this second algorithm, the first previous non-whitespace character is skipped in determining whether the preceding word is a sequence of alphabetic/underscores. This sounds confusing but turns out to be quite practical.
`REPRINT`
  Special character on input and is recognized if the `ICANON` flag is set. Causes the current input edit line to be retyped.
`DSUSP`
  Has similar actions to the `SUSP` character, except that the `SIGTSTP` signal is delivered when one of the processes in the foreground process group issues a read() to the controlling terminal.
`LNEXT`
  Special character on input and is recognized if the `IEXTEN` flag is set. Receipt of this character causes the next character to be taken literally.
`DISCARD`
  Special character on input and is recognized if the `IEXTEN` flag is set. Receipt of this character toggles the flushing of terminal output.
`STATUS`
  Special character on input and is recognized if the `ICANON` flag is set. Receipt of this character causes a `SIGINFO` signal to be sent to the foreground process group of the terminal. Also, if the `NOKERNINFO` flag is not set, it causes the kernel to write a status message to the terminal that displays the current load average, the name of the command in the foreground, its process ID, the symbolic wait channel, the number of user and system seconds used, the percentage of CPU the process is getting, and the resident set size of the process.

The `NL` and `CR` characters cannot be changed. The values for all the remaining characters can be set and are described later in the document under Special Control Characters.

Special character functions associated with changeable special control characters can be disabled individually by setting their value to `_POSIX_VDISABLE`; see Special Control Characters.

If two or more special characters have the same value, the function performed when that character is received is undefined.

## Modem Disconnect

If a modem disconnect is detected by the terminal interface for a controlling terminal, and if `CLOCAL` is not set in the c_cflag field for the terminal, the `SIGHUP` signal is sent to the controlling process associated with the terminal. Unless other arrangements have been made, this causes the controlling process to terminate. Any subsequent call to the read() function returns the value zero, indicating end of file. Thus, processes that read a terminal file and test for end-of-file can terminate appropriately after a disconnect. Any subsequent write() to the terminal device returns -1, with errno set to `EIO`, until the device is closed.

# General Terminal Interface

## Closing a Terminal Device File

The last process to close a terminal device file causes any output to be sent to the device and any input to be discarded. Then, if `HUPCL` is set in the control modes, and the communications port supports a disconnect function, the terminal device performs a disconnect.

## Parameters That Can Be Set

Routines that need to control certain terminal I/O characteristics do so by using the termios structure as defined in the header `<termios.h>`. This structure contains minimally four scalar elements of bit flags and one array of special characters. The scalar flag elements are named: c_iflag, c_oflag, c_cflag, and c_lflag. The character array is named c_cc, and its maximum index is `NCCS`.

## Input Modes

Values of the c_iflag field describe the basic terminal input control, and are composed of following masks:

`IGNBRK`
  /* ignore BREAK condition */
`BRKINT`
  /* map BREAK to SIGINT */
`IGNPAR`
  /* ignore (discard) parity errors */
`PARMRK`
  /* mark parity and framing errors */
`INPCK`
  /* enable checking of parity errors */
`ISTRIP`
  /* strip 8th bit off chars */
`INLCR`
  /* map NL into CR */
`IGNCR`
  /* ignore CR */
`ICRNL`
  /* map CR to NL (ala CRMOD) */
`IXON`
  /* enable output flow control */
`IXOFF`
  /* enable input flow control */
`IXANY`
  /* any char will restart after stop */
`IMAXBEL`
  /* ring bell on input queue full */
`IUCLC`
  /* translate upper case to lower case */

In the context of asynchronous serial data transmission, a break condition is defined as a sequence of zero-valued bits that continues for more than the time to send one byte. The entire sequence of zero-valued bits is interpreted as a single break condition, even if it continues for a time equivalent to more than one byte. In contexts other than asynchronous serial data transmission the definition of a break condition is implementation defined.

If `IGNBRK` is set, a break condition detected on input is ignored, that is, not put on the input queue and therefore not read by any process. If `IGNBRK` is not set and `BRKINT` is set, the break condition flushes the input and output queues and if the terminal is the controlling terminal of a foreground process group, the break condition generates a single `SIGINT` signal to that foreground process group. If neither `IGNBRK` nor `BRKINT` is set, a break condition is read as a single ‘`\0`’, or if `PARMRK` is set, as ‘`\377`’, ‘`\0`’, ‘`\0`’.

If `IGNPAR` is set, a byte with a framing or parity error (other than break) is ignored.

If `PARMRK` is set, and `IGNPAR` is not set, a byte with a framing or parity error (other than break) is given to the application as the three-character sequence ‘`\377`’, ‘`\0`’, X, where ‘`\377`’, ‘`\0`’ is a two-character flag preceding each sequence and X is the data of the character received in error. To avoid ambiguity in this case, if `ISTRIP` is not set, a valid character of ‘`\377`’ is given to the application as ‘`\377`’, ‘`\377`’. If neither `PARMRK` nor `IGNPAR` is set, a framing or parity error (other than break) is given to the application as a single character ‘`\0`’.

If `INPCK` is set, input parity checking is enabled. If `INPCK` is not set, input parity checking is disabled, allowing output parity generation without input parity errors. Note that whether input parity checking is enabled or disabled is independent of whether parity detection is enabled or disabled (see Control Modes). If parity detection is enabled but input parity checking is disabled, the hardware to which the terminal is connected recognizes the parity bit, but the terminal special file does not check whether this bit is set correctly or not.

If `ISTRIP` is set, valid input bytes are first stripped to seven bits, otherwise all eight bits are processed.

If `INLCR` is set, a received `NL` character is translated into a `CR` character. If `IGNCR` is set, a received `CR` character is ignored (not read). If `IGNCR` is not set and `ICRNL` is set, a received `CR` character is translated into a `NL` character.

If `IXON` is set, start/stop output control is enabled. A received `STOP` character suspends output and a received `START` character restarts output. If `IXANY` is also set, then any character may restart output. When `IXON` is set, `START` and `STOP` characters are not read, but merely perform flow control functions. When `IXON` is not set, the `START` and `STOP` characters are read.

If `IXOFF` is set, start/stop input control is enabled. The system shall transmit one or more `STOP` characters, which are intended to cause the terminal device to stop transmitting data, as needed to prevent the input queue from overflowing and causing the undefined behavior described in Input Processing and Reading Data, and shall transmit one or more `START` characters, which are intended to cause the terminal device to resume transmitting data, as soon as the device can continue transmitting data without risk of overflowing the input queue. The precise conditions under which `STOP` and `START` characters are transmitted are implementation defined.

If `IMAXBEL` is set and the input queue is full, subsequent input shall cause an ASCII BEL character to be transmitted to the output queue.

If `IUCLC` is set, characters will be translated from upper to lower case on input.

The initial input control value after open() is implementation defined.

## Output Modes

Values of the c_oflag field describe the basic terminal output control, and are composed of the following masks:

`OPOST`
  /* enable following output processing */
`ONLCR`
  /* map NL to CR-NL (ala `CRMOD`) */
`OXTABS`
  /* expand tabs to spaces */
`ONOEOT`
  /* discard `EOT`'s (^D) on output */
`OCRNL`
  /* map CR to NL */
`OLCUC`
  /* translate lower case to upper case */
`ONOCR`
  /* No CR output at column 0 */
`ONLRET`
  /* NL performs the CR function */

If `OPOST` is set, the remaining flag masks are interpreted as follows; otherwise characters are transmitted without change.

If `ONLCR` is set, newlines are translated to carriage return, linefeeds.

If `OXTABS` is set, tabs are expanded to the appropriate number of spaces (assuming 8 column tab stops).

If `ONOEOT` is set, ASCII EOT characters are discarded on output.

If `OCRNL` is set, carriage returns are translated to newlines.

If `OLCUC` is set, lower case is translated to upper case on output.

If `ONOCR` is set, no CR character is output when at column 0.

If `ONLRET` is set, NL also performs CR on output, and reset current column to 0.

## Control Modes

Values of the c_cflag field describe the basic terminal hardware control, and are composed of the following masks. Not all values specified are supported by all hardware.

`CSIZE`
  /* character size mask */
`CS5`
  /* 5 bits (pseudo) */
`CS6`
  /* 6 bits */
`CS7`
  /* 7 bits */
`CS8`
  /* 8 bits */
`CSTOPB`
  /* send 2 stop bits */
`CREAD`
  /* enable receiver */
`PARENB`
  /* parity enable */
`PARODD`
  /* odd parity, else even */
`HUPCL`
  /* hang up on last close */
`CLOCAL`
  /* ignore modem status lines */
`CCTS_OFLOW`
  /* `CTS` flow control of output */
`CRTSCTS`
  /* same as `CCTS_OFLOW` */
`CRTS_IFLOW`
  /* RTS flow control of input */
`MDMBUF`
  /* flow control output via Carrier */

The `CSIZE` bits specify the byte size in bits for both transmission and reception. The c_cflag is masked with `CSIZE` and compared with the values `CS5`, `CS6`, `CS7`, or `CS8`. This size does not include the parity bit, if any. If `CSTOPB` is set, two stop bits are used, otherwise one stop bit. For example, at 110 baud, two stop bits are normally used.

If `CREAD` is set, the receiver is enabled. Otherwise, no character is received. Not all hardware supports this bit. In fact, this flag is pretty silly and if it were not part of the `termios` specification it would be omitted.

If `PARENB` is set, parity generation and detection are enabled and a parity bit is added to each character. If parity is enabled, `PARODD` specifies odd parity if set, otherwise even parity is used.

If `HUPCL` is set, the modem control lines for the port are lowered when the last process with the port open closes the port or the process terminates. The modem connection is broken.

If `CLOCAL` is set, a connection does not depend on the state of the modem status lines. If `CLOCAL` is clear, the modem status lines are monitored.

Under normal circumstances, a call to the open() function waits for the modem connection to complete. However, if the `O_NONBLOCK` flag is set or if `CLOCAL` has been set, the open() function returns immediately without waiting for the connection.

If `CCTS_OFLOW` (`CRTSCTS`) is set, transmission is stopped when `CTS` is lowered and resumed when `CTS` is raised.

If `MDMBUF` is set then output flow control is controlled by the state of Carrier Detect.

If the object for which the control modes are set is not an asynchronous serial connection, some of the modes may be ignored; for example, if an attempt is made to set the baud rate on a network connection to a terminal on another host, the baud rate may or may not be set on the connection between that terminal and the machine it is directly connected to.

## Local Modes

Values of the c_lflag field describe the control of various functions, and are composed of the following masks.

`ECHOKE`
  /* visual erase for line kill */
`ECHOE`
  /* visually erase chars */
`ECHOK`
  /* echo NL after line kill */
`ECHO`
  /* enable echoing */
`ECHONL`
  /* echo `NL` even if `ECHO` is off */
`ECHOPRT`
  /* visual erase mode for hardcopy */
`ECHOCTL`
  /* echo control chars as ^(Char) */
`ISIG`
  /* enable signals `INTR`, `QUIT`, `[D]SUSP` */
`ICANON`
  /* canonicalize input lines */
`ALTWERASE`
  /* use alternate `WERASE` algorithm */
`IEXTEN`
  /* enable `DISCARD` and `LNEXT` */
`EXTPROC`
  /* external processing */
`TOSTOP`
  /* stop background jobs from output */
`FLUSHO`
  /* output being flushed (state) */
`NOKERNINFO`
  /* no kernel output from `VSTATUS` */
`PENDIN`
  /* XXX retype pending input (state) */
`NOFLSH`
  /* don't flush after interrupt */
`XCASE`
  /* canonical upper/lower case */

If `ECHO` is set, input characters are echoed back to the terminal. If `ECHO` is not set, input characters are not echoed.

If `ECHOE` and `ICANON` are set, the `ERASE` character causes the terminal to erase the last character in the current line from the display, if possible. If there is no character to erase, an implementation may echo an indication that this was the case or do nothing.

If `ECHOK` and `ICANON` are set, the `KILL` character causes the current line to be discarded and the system echoes the ‘`\n`’ character after the `KILL` character.

If `ECHOKE` and `ICANON` are set, the `KILL` character causes the current line to be discarded and the system causes the terminal to erase the line from the display.

If `ECHOPRT` and `ICANON` are set, the system assumes that the display is a printing device and prints a backslash and the erased characters when processing `ERASE` characters, followed by a forward slash.

If `ECHOCTL` is set, the system echoes control characters in a visible fashion using a caret followed by the control character.

If `ALTWERASE` is set, the system uses an alternative algorithm for determining what constitutes a word when processing `WERASE` characters (see `WERASE`).

If `ECHONL` and `ICANON` are set, the ‘`\n`’ character echoes even if `ECHO` is not set.

If `ICANON` is set, canonical processing is enabled. This enables the erase and kill edit functions, and the assembly of input characters into lines delimited by `NL`, `EOF`, and `EOL`, as described in Canonical Mode Input Processing.

If `ICANON` is not set, read requests are satisfied directly from the input queue. A read is not satisfied until at least `VMIN` bytes have been received or the timeout value `VTIME` expired between bytes. The time value represents tenths of seconds. See Noncanonical Mode Input Processing for more details.

If `ISIG` is set, each input character is checked against the special control characters `INTR`, `QUIT`, and `SUSP` (job control only). If an input character matches one of these control characters, the function associated with that character is performed. If `ISIG` is not set, no checking is done. Thus these special input functions are possible only if `ISIG` is set.

If `IEXTEN` is set, implementation-defined functions are recognized from the input data. How `IEXTEN` being set interacts with `ICANON`, `ISIG`, `IXON`, or `IXOFF` is implementation defined. If `IEXTEN` is not set, then implementation-defined functions are not recognized, and the corresponding input characters are not processed as described for `ICANON`, `ISIG`, `IXON`, and `IXOFF`.

If `NOFLSH` is set, the normal flush of the input and output queues associated with the `INTR`, `QUIT`, and `SUSP` characters is not done.

If `XCASE` and `ICANON` is set, an upper case character is preserved on input if prefixed by a \ character. In addition, this prefix is added to upper case characters on output.

In addition, the following special character translations are in effect:

for: | use:
``` | \'
`|` | \!
`~` | \^
`{` | \(
`}` | \)
`\` | \\

If `TOSTOP` is set, the signal `SIGTTOU` is sent to the process group of a process that tries to write to its controlling terminal if it is not in the foreground process group for that terminal. This signal, by default, stops the members of the process group. Otherwise, the output generated by that process is output to the current output stream. Processes that are blocking or ignoring `SIGTTOU` signals are excepted and allowed to produce output and the `SIGTTOU` signal is not sent.

If `NOKERNINFO` is set, the kernel does not produce a status message when processing `STATUS` characters (see `STATUS`).

## Special Control Characters

The special control characters values are defined by the array c_cc. This table lists the array index, the corresponding special character, and the system default value. For an accurate list of the system defaults, consult the header file `<sys/ttydefaults.h>`.

Index Name | Special Character | Default Value
`VEOF` | EOF | ^D
`VEOL` | EOL | _POSIX_VDISABLE
`VEOL2` | EOL2 | _POSIX_VDISABLE
`VERASE` | ERASE | ^? ‘`\177`’
`VWERASE` | WERASE | ^W
`VKILL` | KILL | ^U
`VREPRINT` | REPRINT | ^R
`VINTR` | INTR | ^C
`VQUIT` | QUIT | ^\\ ‘`\34`’
`VSUSP` | SUSP | ^Z
`VDSUSP` | DSUSP | ^Y
`VSTART` | START | ^Q
`VSTOP` | STOP | ^S
`VLNEXT` | LNEXT | ^V
`VDISCARD` | DISCARD | ^O
`VMIN` | --- | 1
`VTIME` | --- | 0
`VSTATUS` | STATUS | ^T

If the value of one of the changeable special control characters (see Special Characters) is `_POSIX_VDISABLE`, that function is disabled; that is, no input data is recognized as the disabled special character. If `ICANON` is not set, the value of `_POSIX_VDISABLE` has no special meaning for the `VMIN` and `VTIME` entries of the c_cc array.

The initial values of the flags and control characters after open() is set according to the values in the header `<sys/ttydefaults.h>`.

# SEE ALSO

tcgetattr(3), tcsetattr(3)

November 9, 2021 | Debian