ASTFB(4) | Device Drivers Manual (powerpc64) | ASTFB(4)

# NAME

`astfb` — Aspeed BMC frame buffer

# SYNOPSIS

`astfb* at pci?`
`wsdisplay* at astfb?`

# DESCRIPTION

The `astfb` driver supports the frame buffer set up by firmware on systems with an Aspeed Baseboard Management Controller (BMC).

The `astfb` driver interfaces the frame buffer with the wscons(4) console framework. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# SEE ALSO

intro(4), wscons(4), wsdisplay(4)

# HISTORY

The `astfb` driver first appeared in OpenBSD 6.9.

# AUTHORS

The `astfb` driver was written by Mark Kettenis <kettenis@openbsd.org>.

October 3, 2020 | Debian