NEO(4) | Device Drivers Manual | NEO(4)

# NAME

`neo` — NeoMagic 256AV/ZX audio device

# SYNOPSIS

`neo* at pci?`
`audio* at neo?`

# DESCRIPTION

The `neo` driver provides support for NeoMagic MagicMedia 256AV and 256ZX audio chips found in many laptops, and perhaps on some PCI cards.

# FILES

The driver needs a firmware file, which is loaded on demand when the device is attached:

/etc/firmware/neo-coefficients

# SEE ALSO

ac97(4), audio(4), intro(4), pci(4)

# HISTORY

The `neo` device driver appeared in OpenBSD 2.7.

# BUGS

This driver has some bugs because NeoMagic refuses to provide documentation, even though they are discontinuing their products. At the time of contact, all persons working at the company were hiding behind their receptionist as if in a stage of siege.

September 11, 2023 | Debian