RAPTOR(4) | Device Drivers Manual (sparc64) | RAPTOR(4)

# NAME

`raptor` — accelerated color frame buffer

# SYNOPSIS

`raptor* at pci?`
`wsdisplay* at raptor?`

# DESCRIPTION

The `raptor` driver supports Tech Source Raptor PCI frame buffer cards based on the Number 9 ‘Imagine-128’ chips, such as the Tech Source Raptor GFX-4M and Raptor GFX-8M boards. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# SEE ALSO

intro(4), pci(4), wscons(4), wsdisplay(4)

February 24, 2011 | Debian