OMAP(4) | Device Drivers Manual (armv7) | OMAP(4)

# NAME

`omap` — omap3, omap4, am335x SoCs device bus

# SYNOPSIS

`omap0 at mainbus?`

# DESCRIPTION

The `omap` interface serves as an abstraction used by the autoconfiguration system to help find and attach devices integrated on Texas Instruments SoC processors.

`omap` provides support for the following devices:

dmtimer(4)
  Texas Instruments dual mode timer device
gptimer(4)
  Texas Instruments general purpose timer device
prcm(4)
  Texas Instruments power, reset and clock management device

# SEE ALSO

intro(4), mainbus(4)

# HISTORY

The `omap` driver first appeared in OpenBSD 5.5.

April 5, 2020 | Debian