UFTDI(4) | Device Drivers Manual | UFTDI(4)

# NAME

`uftdi` — FTDI USB serial adapter

# SYNOPSIS

`uftdi* at uhub?`
`ucom* at uftdi?`

# DESCRIPTION

The `uftdi` driver provides support for various serial adapters based on the FTDI FT8U100AX, FT8U232AM, FT8U245AM, FT232B/H/R, FT245B/R, FT2232C/D/H/L, FT4232H and FT-X series chips.

The device is accessed through the ucom(4) driver which makes it behave like a tty(4).

# SEE ALSO

intro(4), tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `uftdi` driver appeared in NetBSD 1.5. OpenBSD support was added in OpenBSD 2.9.

January 12, 2014 | Debian