UARK(4) | Device Drivers Manual | UARK(4)

# NAME

`uark` — Arkmicro Technologies ARK3116 based USB serial adapter

# SYNOPSIS

`uark* at uhub?`
`ucom* at uark?`

# DESCRIPTION

The `uark` driver supports Arkmicro Technologies ARK3116 based serial adapters.

The following devices should work with the `uark` driver:

    HL USB-RS232
    HugePine USB-UART
    KQ-U8A Data Cable
    Skymaster USB to RS232

# SEE ALSO

tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `uark` device driver first appeared in OpenBSD 4.0.

# AUTHORS

The `uark` driver was written by Jonathan Gray <jsg@openbsd.org>.

# CAVEATS

Setting hardware flow control is not currently supported. It is not yet known how to ask the hardware to send a break.

Arkmicro Technologies do not reply to requests of documentation for their products.

July 16, 2013 | Debian