AMLRESET(4) | Device Drivers Manual | AMLRESET(4)

# NAME

`amlreset` — Amlogic reset controller

# SYNOPSIS

`amlreset* at fdt?`

# DESCRIPTION

The `amlreset` driver controls the reset signals for integrated components of Amlogic SoCs.

# SEE ALSO

amlclock(4), intro(4)

# HISTORY

The `amlreset` device driver first appeared in OpenBSD 6.6.

# AUTHORS

The `amlreset` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 27, 2019 | Debian