HILID(4) | Device Drivers Manual | HILID(4)

# NAME

`hilid` — HIL ID module device

# SYNOPSIS

`hilid* at hil?`

# DESCRIPTION

This driver recognizes the HIL “ID module” device. The only purpose of this device is to provide a small, unique, bitstring.

# SEE ALSO

hil(4), intro(4)

# BUGS

There is currently no way to communicate the ID module bitstring to userland applications.

May 31, 2007 | Debian