GDT(4) | Device Drivers Manual | GDT(4)

# NAME

`gdt` — ICP-Vortex and Intel GDT SATA/SCSI RAID controller

# SYNOPSIS

`gdt* at pci?`

# DESCRIPTION

The `gdt` driver provides support for ICP-Vortex adapters such as:

GDT4x13RZ, GDT4x23RZ, GDT6000/6020/6050, GDT6000B/6010, GDT6110/6510, GDT6120/6520, GDT6513RS, GDT6518RS, GDT6523RS, GDT6530, GDT6535, GDT6537, GDT6537RP, GDT6537RP1, GDT6537RP2, GDT6550, GDT6555, GDT6557, GDT6557RP, GDT6557RP1, GDT6557RP2, GDT6x11RP, GDT6x11RP1, GDT6x11RP2, GDT6x15, GDT6x17, GDT6x17RP, GDT6x17RP1, GDT6x17RP2, GDT6x18RD, GDT6x19RD, GDT6x21RP, GDT6x21RP1, GDT6x21RP2, GDT6x25, GDT6x27, GDT6x27RP, GDT6x27RP1, GDT6x27RP2, GDT6x28RD, GDT6x28RS, GDT6x29RD, GDT6x33RS, GDT6x38RD, GDT6x38RS, GDT6x43RS, GDT6x53RS, GDT6x58RD, GDT6x58RS, GDT6x63RS, GDT7x13RN, GDT7x18RN, GDT7x19RN, GDT7x23RN, GDT7x28RN, GDT7x29RN, GDT7x38RN, GDT7x43RN, GDT7x53RN, GDT7x58RN, GDT7x63RN, GDT8x00RZ, GDT8x13RZ, GDT8x14RZ, GDT8x22RZ, GDT8x23RZ, GDT8x24RZ, GDT8x33RZ, GDT8x43RZ, GDT8x46RZ, GDT8x53RZ, GDT8x63RZ, and GDT8x86RZ.

As well as Intel adapters such as:

SRCU42L, SRCU32, SRCZCR, and SRCS14L.

Although the controllers are actual RAID controllers, the driver makes them look just like SCSI controllers. All RAID configuration is done through the controllers' BIOSes.

# DIAGNOSTICS

pci_mem_find: expected mem type 00000000, found 00000002
  This message occurs during autoconfiguration if jumper J4 is set to map the controller memory below 1MB in physical memory. The driver primarily wants this jumper to be set the other way round, but it will work with it in any setting. If the diagnostic is considered a nuisance, alter jumper J4's setting.

# SEE ALSO

intro(4), pci(4), scsi(4), sd(4)

# HISTORY

The `gdt` driver first appeared in OpenBSD 2.7.

# AUTHORS

The `gdt` driver was written by Niklas Hallqvist <niklas@openbsd.org>, inspired by the Linux driver by Achim Luebner <achim@vortex.de>.

# BUGS

An ISA & EISA front-end is needed.

The driver does not support transparent raw SCSI mode.

It would be nice to configure the RAID units after boot but the information on how to do that is not public.

April 12, 2023 | Debian