CREATOR(4) | Device Drivers Manual (sparc64) | CREATOR(4)

# NAME

`creator` — accelerated color frame buffer

# SYNOPSIS

`creator* at mainbus0 flags 0x0`
`creator* at upa0 flags 0x0`
`wsdisplay* at creator?`

# DESCRIPTION

The Creator, Creator 3D and Elite 3D are color frame buffers, with graphics acceleration, available for most of the UltraSPARC workstations with UPA slots.

The `creator` driver interfaces those frame buffers with the wscons(4) console framework. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

By default hardware acceleration is used to erase the screen and scroll text. By setting flags to 1 (via config(8) or boot_config(8)) this acceleration can be disabled.

# SEE ALSO

intro(4), upa(4), wscons(4), wsdisplay(4), boot_config(8), config(8)

November 26, 2010 | Debian