QLE(4) | Device Drivers Manual | QLE(4)

# NAME

`qle` — QLogic ISP2400/2500 Fibre Channel controller

# SYNOPSIS

`qle* at pci?`

# DESCRIPTION

The `qle` driver provides support for 4G and 8G QLogic Fibre Channel host bus adapters using the ISP2400 and ISP2500 family of chipsets.

`qle` provides no ability to configure an adapter's parameters at runtime; all configuration must be done prior to booting OpenBSD.

# SEE ALSO

intro(4), pci(4), qla(4), qlw(4), scsi(4)

# HISTORY

The `qle` driver first appeared in OpenBSD 5.5.

# AUTHORS

The `qle` driver was written by Jonathan Matthew <jmatthew@openbsd.org>.

January 21, 2015 | Debian