WBNG(4) | Device Drivers Manual | WBNG(4)

# NAME

`wbng` — Winbond W83793G temperature, voltage, and fan sensor

# SYNOPSIS

`wbng* at iic?`

# DESCRIPTION

The `wbng` driver provides support for the Winbond W83793G Hardware Monitor. The device provides 10 voltage sensors, 6 temperature sensors and 12 fan sensors. Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `wbng` driver first appeared in OpenBSD 4.3.

# AUTHORS

The `wbng` driver was written by Constantine A. Murenin <cnst@openbsd.org>.

July 16, 2013 | Debian