GFXP(4) | Device Drivers Manual (sparc64) | GFXP(4)

# NAME

`gfxp` — accelerated color frame buffer

# SYNOPSIS

`gfxp* at pci?`
`wsdisplay* at gfxp?`

# DESCRIPTION

The `gfxp` driver supports Tech Source Raptor PCI frame buffer cards based on the 3D Labs ‘Permedia v2’ chips, such as the Sun PGX32 and Tech Source Raptor GFX-8P boards. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# SEE ALSO

intro(4), pci(4), wscons(4), wsdisplay(4)

October 27, 2009 | Debian