SMSC(4) | Device Drivers Manual | SMSC(4)

# NAME

`smsc` — SMSC LAN95xx 10/100 USB Ethernet device

# SYNOPSIS

`smsc* at uhub?`

# DESCRIPTION

The `smsc` driver supports SMSC LAN9500/LAN9500A/LAN9530/LAN9730/LAN89530 USB 2.0 10/100 Ethernet devices and LAN951x USB 2.0 hub and 10/100 Ethernet devices, including:

Gamber Johnson MAG Docking Station 7160-0204
Gamber Johnson MAG Docking Station 7160-0205
Gamber Johnson MAG Docking Station 7160-0227
GWC Technology HE2440
HP USB Media Port Replicator
j5create Newport Station JUD200
Kensington Universal Notebook Docking Station (K33926US)
LevelOne USB-0501
Samsung Central Station monitors
StarTech USBVGADOCK2
XPower XP2440

For more information on configuring this device, see ifconfig(8).

# SEE ALSO

arp(4), ifmedia(4), mii(4), netintro(4), uhub(4), usb(4), hostname.if(5), ifconfig(8)

# HISTORY

The `smsc` device driver first appeared in OpenBSD 5.3.

# AUTHORS

The `smsc` driver was written by Ben Gray <bgray@freebsd.org>.

April 8, 2014 | Debian