QLA(4) | Device Drivers Manual | QLA(4)

# NAME

`qla` — QLogic ISP2100/2200/2300 Fibre Channel controller

# SYNOPSIS

`qla* at pci?`
`qla* at sbus?`

# DESCRIPTION

The `qla` driver provides support for 1G and 2G QLogic Fibre Channel host bus adapters using the ISP2100, ISP2200, and ISP2300 chipsets.

`qla` provides no ability to configure an adapter's parameters at runtime; all configuration must be done prior to booting OpenBSD.

# SEE ALSO

intro(4), pci(4), qle(4), qlw(4), sbus(4), scsi(4)

# HISTORY

The `qla` driver first appeared in OpenBSD 5.5.

# AUTHORS

The `qla` driver was written by Jonathan Matthew <jmatthew@openbsd.org>.

March 16, 2014 | Debian