GEODESC(4) | Device Drivers Manual (i386) | GEODESC(4)

# NAME

`geodesc` — Geode SC1100/SCx200 IAOC watchdog timer device

# SYNOPSIS

`geodesc* at pci?`

# DESCRIPTION

The `geodesc` driver supports the watchdog timer of the Geode SC1100.

The Geode SC1100/SCx200 is a member of the AMD Information Appliance On a Chip (IAOC) family of fully integrated x86 system chips.

The watchdog timer may be configured via sysctl(8).

# SEE ALSO

watchdog(4), sysctl(8)

# HISTORY

Support for the `geodesc` was added in OpenBSD 3.4.

# AUTHORS

The `geodesc` driver was written by Markus Friedl.

May 31, 2007 | Debian