GSCKBC(4) | Device Drivers Manual (hppa) | GSCKBC(4)

# NAME

`gsckbc` — PS/2-like controller driver

# SYNOPSIS

`gsckbc* at gsc? irq 26`
`pckbd* at gsckbc?`
`pms* at gsckbc?`

# DESCRIPTION

The `gsckbc` driver handles resource allocation and device attachment for the PS/2 input device ports. Each `gsckbc` driver provides the logical connection for one child device, either the “keyboard” port or the “mouse” port.

# SEE ALSO

gsc(4), pckbd(4), pms(4)

July 16, 2008 | Debian