IMXTEMP(4) | Device Drivers Manual (armv7) | IMXTEMP(4)

# NAME

`imxtemp` — i.MX6 temperature monitor

# SYNOPSIS

`imxtemp* at fdt?`

# DESCRIPTION

The `imxtemp` driver provides support for the temperature sensor found on the Freescale i.MX6 SoC processors.

Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `imxtemp` driver first appeared in OpenBSD 6.1.

# AUTHORS

The `imxtemp` driver was written by Patrick Wildt <patrick@blueri.se> and Mark Kettenis <kettenis@openbsd.org>.

June 20, 2020 | Debian