BCMTEMP(4) | Device Drivers Manual | BCMTEMP(4)

# NAME

`bcmtemp` — Broadcom BCM2835/BCM2836/BCM2837 temperature monitor

# SYNOPSIS

`bcmtemp* at fdt?`

# DESCRIPTION

The `bcmtemp` driver provides support for the temperature sensor found on the Broadcom BCM2835/BCM2836/BCM2837 SoC.

Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `bcmtemp` driver first appeared in OpenBSD 6.3.

# AUTHORS

The `bcmtemp` driver was written by Mark Kettenis <kettenis@openbsd.org>.

June 20, 2020 | Debian