SPC(4) | Device Drivers Manual (luna88k) | SPC(4)

# NAME

`spc` — Fujitsu MB87030/MB89352 SCSI device

# SYNOPSIS

`spc0 at mainbus0`
`spc1 at mainbus0`

# DESCRIPTION

The `spc` driver provides support for the Fujitsu MB87030/MB89352 SCSI Protocol Controller (SPC) chips.

# SEE ALSO

cd(4), ch(4), intro(4), scsi(4), sd(4), st(4), uk(4)

# BUGS

Synchronous data transfers are not currently supported.

August 14, 2012 | Debian