UGURU(4) | Device Drivers Manual | UGURU(4)

# NAME

`uguru` — ABIT temperature, voltage and fan sensors

# SYNOPSIS

`uguru0 at isa? port 0xe0`

# DESCRIPTION

The `uguru` driver provides support for the microcontroller found in various ABIT motherboards which serves as the gateway chip between system management software and hardware. Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

intro(4), isa(4), sensorsd(8), sysctl(8)

# HISTORY

The `uguru` driver first appeared in OpenBSD 4.8

# AUTHORS

The `uguru` driver was written by Mikko Tolmunen <oskari@sefirosu.org>.

# BUGS

Interrupt support is unimplemented.

July 16, 2013 | Debian