BSD.RE-CONFIG(5) | File Formats Manual | BSD.RE-CONFIG(5)

# NAME

`bsd.re-config` — kernel configuration file

# DESCRIPTION

The `bsd.re-config` file contains kernel modification commands in config(8) format. If present, it is used during system startup to configure the kernel that will be running at the next boot. It can be used to enable or disable specific devices in the kernel.

# FILES

/etc/bsd.re-config
  Kernel configuration file.

# EXAMPLES

To enable the ipmi(4) driver, add the following line to `bsd.re-config`:

`enable ipmi`

# SEE ALSO

config(8)

May 31, 2025 | Debian