RADIUSD(8) | System Manager's Manual | RADIUSD(8)

# NAME

`radiusd` — Remote Authentication Dial In User Service (RADIUS) daemon

# SYNOPSIS

`radiusd` | [`-dn`] [`-f` file]

# DESCRIPTION

The `radiusd` daemon implements the RADIUS protocol.

To have `radiusd` enabled at boot time, use “rcctl enable radiusd”, which sets

`radiusd_flags=""`

in rc.conf.local(8).

The options are as follows:

`-d`
  Do not daemonize, log to `stderr` instead of syslog(3), and produce some additional debugging output.
`-f` file
  Specify an alternative configuration file.
`-n`
  Configtest mode. Only check the configuration file for validity.

# FILES

/etc/radiusd.conf
  Default configuration file.

# SEE ALSO

radiusd.conf(5), radiusctl(8), rc.conf(8)

# STANDARDS

Remote Authentication Dial In User Service (RADIUS), RFC 2865, June 2000.

# HISTORY

The `radiusd` daemon first appeared in OpenBSD 5.8.

# AUTHORS

YASUOKA Masahiko <yasuoka@openbsd.org>

November 10, 2019 | Debian