SNMPD_METRICS(8) | System Manager's Manual | SNMPD_METRICS(8)

# NAME

`snmpd_metrics` — export snmpd MIB data

# SYNOPSIS

`snmpd_metrics` | [`-dv`] [`-C` option] [`-c` context] [`-s` path]

# DESCRIPTION

`snmpd_metrics` exports the following (partial) MIBs via an AgentX compatible (snmp) daemon: HOST-RESOURCES-MIB, IF-MIB, OPENBSD-PF-MIB, OPENBSD-SENSORS-MIB, OPENBSD-CARP-MIB, OPENBSD-MEM-MIB, IP-MIB, IP-FORWARD-MIB, UCD-DISKIO-MIB, and BRIDGE-MIB.

The options are as follows:

`-C` option
  Enable MIB-specific options. Currently only `filter-routes` is supported. If set ask the kernel to filter route update messages on the routing socket. Routing table information will not be available, but CPU use will be reduced during bulk updates.
`-c` context
  The SNMPv3 context and can usually be omitted.
`-d`
  Do not daemonize and log to stderr.
`-s` path
  Connect to the AgentX master via path. It defaults to /var/agentx/master.
`-v`
  Produce more verbose output.

# SEE ALSO

snmp(1), snmpd(8)

# STANDARDS

P. Grillo and WeSync.com, Host Resources MIB, RFC 2790, March 2000.

K. McCloghrie, Cisco Systems, F. Kastenholz, and Argon Networks, The Interfaces Group MIB, RFC 2863, June 2000.

S. Routhier, Ed., Management Information Base for the Internet Protocol (IP), RFC 4293, April 2006.

B. Haberman and Johns Hopkins University, IP Forwarding Table MIB, RFC 4292, April 2006.

K. Norseth, Ed., L-3 Communications, E. Bell, Ed., and 3Com Europe Limited, Definitions of Managed Objects for Bridges, RFC 4188, September 2005.

# AUTHORS

Martijn van Duren <martijn@openbsd.org>
Joel Knight <joel@openbsd.org>
Reyk Floeter <reyk@openbsd.org>

October 23, 2022 | Debian